ORAMA AXIS

The Pivoting Frame

The door swings around an asymmetrically located axis, creating a short-lasting anti-gravity moment. AXIS gently opens with a simple and effortless push.

Specifications

Maximum Leaf Height up to 6,5 m

Maximum Leaf Width up to 3 m

Glass Thickness from 30 to 54mm

Maximun Leaf Weight up to 1000 kg

AXIS Glazing   
  
Omicron – Standards double glazing option, forming minimal profiles and providing maximum comfort.